**GALVANIC SKIN RESPONSE METER**

**Model GS-01**

Technical data:

* Processor: **Risk-based microcontroller**
* Sampling rate: **1Hz – 800Hz**
* Output voltage: less than **3,9V**
* Range: **0,488 – 35µS**
* Precision class: **1%**
* Power supply and connection: **USB**
* Power: **0,5W**
* Size: **90х50х15**mm (as a match box)
* Weight: **60g**

Price:

* 145.00EUR (for single device incl. sensors and USB cable)

Warranty:

* 2 years

Developed by Eng. Dobrin Ivanov (dobalekt@gmail.com) for Sofia University, © 2017.

04-05-2017